HYMN-1-100 hymn board consisting of:

High-quality LED display hymn board type: HYMN-1-100 particularly suitable for churches, latest technology with the highest functional standard. The HYMN-1-100 model is a 2-line display for song number and verse with 5 display digits each. The high-resolution LED matrix with 6100 pixels integrated into the hymn boards ensures excellent readability, even from long distances. A special surface technology prevents any reflections, and even lamps or light-flooded rooms do not affect readability. The control is via tablet/APP (smartphone) and/or radio input device, radio receiver with internal antenna is built in. Model Type: HYMN-1-100 APP is equipped with its own ACCESS POINT WLAN system adapter. This means that no WiFi / WLAN is required on site. Individual automatic brightness control for each hymn board, according to the respective light incidence. The display color can be freely selected by the operator via tablet/APP or input device and changed at any time. There is also a separate color selection for lines 1 and 2. There is a run-through before the service with 20 storage locations. Any number of HYMN-M expansion modules can be added. Optionally wall or tripod mounting are possible. Tripod solution with battery pack also suitable for listed buildings. Power supply: Optionally via a power supply 12VDC to 24VDC / 2.1 mm barrel plug 1.5A or battery pack. Dimensions: L=387mm x W=257mm x D=30mm. Digit height: 100mm. Reading distance: up to 40 meters

Deliver, assemble, connect

**Brand:** Phoenix Professional Audio

**Type:** HYMN-1-100