HYMN-MSH motor swivel mount consisting of:

The motor swivel mount is particularly suitable for the hymn boards of the HYMN series. The electric drive of the wall swivel holder is particularly quiet in operation. The boom can be used on one or both sides with a 90 degree swivel range. Automatic control, unfolding and retraction takes place via tablet/APP/hymn board or input device. One-time basic setting is carried out using the included IR remote control. Total dimensions W=630 mm to 990 mm, wall plate W=110 mm x H=310 mm, holding profiles W=30 mm x H=435 mm. Color white. Noise level: low. Power supply: External power supply 12VDC.

Deliver, assemble, connect

**Brand:** Phoenix Professional Audio

**Type:** HYMN-MSH